{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Sheet1","zRef_Drop_Downs","Directions","Max","30 Day","MonRoundInfo"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":1,"defined_names":12,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"zRef_Drop_Downs","index":1,"n_rows":1,"n_cols":3,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Table","Column","Values"]

{"sheet":"Directions","index":2,"n_rows":26,"n_cols":2,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
[]
[null,"These Guidelines have been transposed from the original.  Last Update March 2016"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Disclaimer: All care has been exercised in the compilation of these guidelines for quick import to ESDAT, however no liability is taken for any error.  It is the responsibility of the user to review the contained data and ensure their data is compliant with the relevant guidelines, and that this compilation meets their requirements.  "]
[]
[]
[null,"These Guidelines require ESdat 5 or later"]
[]
[]
[]
[]
[]
[null,"This data is compiled into the ESdat \"Standards Production Wizard\" which is used to generate Import Templates for more complex environmental standards"]
[]
[null,"The import process is:"]
[null,"1. Use the Standards Production Wizard sheet to generate an ESdat Import Template.  "]
[null,"2. Import the standards into ESdat."]

{"sheet":"Max","index":3,"n_rows":291,"n_cols":17,"rows_kept":291,"cut":false,"hidden":false,"merged":[]}
["Project:","|All","0|0","Table:","[zRef_Environmental_Standards]",null,"Style:","EnviroStandards","HasLocs"]
["ODBC:","FileDSN=C:\\Users\\nicktumney.EARTHSCIENCE\\Documents\\_ESdat\\esdatonline-ca.dsn;UID=?UID;Password=3CvpNGg4;Trusted_Connection=no",null,"Parent Tables:","zRef_Matrix_Types,zRef_Chemistry_Lookup",null,"OnlineBaseURL:","http://online-ca.esdat.net"]
["|All"]
["ChemCode","ChemName","MatrixType","ActionLevelSource","ActionLevel","ActionLevel_Min","Units","Comments","ActionLevel_Prefix","Conditional_ChemCode1","Conditional_ChemCode1_Units","Conditional_ChemCode1_Min_Value_Prefix","Conditional_ChemCode1_Value_Min","Conditional_ChemCode1_Max_Value_Prefix","Conditional_ChemCode1_Value_Max","Applies_To_Total_Result","Applies_To_Filtered_Result"]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Drinking Water Supply (30 day)",5000,null,"ug/L"]
["100-41-4","Ethylbenzene","Water","BC Approved WQG - Drinking Water Supply (Max)",2.3999999999999998E-3,null,"mg/L"]
["120-83-2","2,4-dichlorophenol","Water","BC Approved WQG - Drinking Water Supply (Max)",900,null,"ug/L"]
["14797-55-8(as N)","Nitrate as N","Water","BC Approved WQG - Drinking Water Supply (Max)",10,null,"mg/L"]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Drinking Water Supply (Max)",1,null,"mg/L"]
["14808-79-8","Sulphate","Water","BC Approved WQG - Drinking Water Supply (Max)",500,null,"mg/L"]
["14866-68-3","Chlorate","Water","BC Approved WQG - Drinking Water Supply (Max)",2.4,null,"mg/L"]
["1634-04-4","Methyl Tertiary-Butyl Ether","Water","BC Approved WQG - Drinking Water Supply (Max)",0.02,null,"mg/L"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Drinking Water Supply (Max)",1.5,null,"mg/L"]
["50-32-8","Benzo[a]pyrene","Water","BC Approved WQG - Drinking Water Supply (Max)",0.01,null,"µg/L"]
["58-90-2","2,3,4,6-tetrachlorophenol","Water","BC Approved WQG - Drinking Water Supply (Max)",60,null,"ug/L"]
["71-43-2","Benzene","Water","BC Approved WQG - Drinking Water Supply (Max)",5,null,"ug/L"]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Drinking Water Supply (Max)",0.2,null,"mg/L",null,null,null,null,null,null,null,null,false,true]
["7439-92-1","Lead","Water","BC Approved WQG - Drinking Water Supply (Max)",50,null,"ug/L"]
["7439-97-6","Mercury","Water","BC Approved WQG - Drinking Water Supply (Max)",1,null,"ug/L"]
["7439-98-7","Molybdenum","Water","BC Approved WQG - Drinking Water Supply (Max)",0.25,null,"mg/L"]
["7440-38-2","Arsenic (total)","Water","BC Approved WQG - Drinking Water Supply (Max)",25,null,"ug/L"]
["7440-42-8","Boron","Water","BC Approved WQG - Drinking Water Supply (Max)",5,null,"mg/L"]
["7440-50-8","Copper (total)","Water","BC Approved WQG - Drinking Water Supply (Max)",500,null,"ug/L"]
["7723-14-0","Phosphorous","Water","BC Approved WQG - Drinking Water Supply (Max)",10,null,"ug/L"]
["7782-49-2","Selenium","Water","BC Approved WQG - Drinking Water Supply (Max)",10,null,"ug/L"]
["88-06-2","2,4,6-trichlorophenol ","Water","BC Approved WQG - Drinking Water Supply (Max)",5,null,"ug/L"]
["Colour","Colour","Water","BC Approved WQG - Drinking Water Supply (Max)",15,null,"mg/L Pt","True Color"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Drinking Water Supply (Max)",0,null,"num/100mL","No treatment"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Drinking Water Supply (Max)",10,null,"num/100mL","Disinfection only - 90th precentile","≤"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Drinking Water Supply (Max)",100,null,"num/100mL","Partial treatment - 90th pertcentile","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Drinking Water Supply (Max)",0,null,"num/100mL","No treatment"]
["Enterococci","Enterococci","Water","BC Approved WQG - Drinking Water Supply (Max)",3,null,"num/100mL","Disinfection only - 90th precentile","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Drinking Water Supply (Max)",25,null,"num/100mL","Partial treatment - 90th pertcentile","≤"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Drinking Water Supply (Max)",0,null,"num/100mL","No treatment"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Drinking Water Supply (Max)",10,null,"num/100mL","Disinfection only - 90th precentile","≤"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Drinking Water Supply (Max)",100,null,"num/100mL","Partial treatment - 90th pertcentile","≤"]
["NO3+NO2 (as N)","Nitrite + Nitrate as N","Water","BC Approved WQG - Drinking Water Supply (Max)",10,null,"mg/L"]
["Pseudomonasaeruginos","Pseudomonas aeruginosa","Water","BC Approved WQG - Drinking Water Supply (Max)",0,null,"num/100mL","No treatment"]
["SAD_CYANIDE","Strong-acid Dissociable Cyanide Plus Thiocyanate","Water","BC Approved WQG - Drinking Water Supply (Max)",200,null,"ug/L"]
["Temp","Temperature","Water","BC Approved WQG - Drinking Water Supply (Max)",15,null,"oC"]
["TOC","Organic Carbon","Water","BC Approved WQG - Drinking Water Supply (Max)",4,null,"mg/L"]
["TURBIDITY","Turbidity","Water","BC Approved WQG - Drinking Water Supply (Max)",null,null,"NTU","Compare to Background"]
["100-41-4","Ethylbenzene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.2,null,"mg/L"]
["108-46-3","3-hydroxyphenol (resorcinol)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",12.5,null,"ug/L"]
["108-88-3","Toluene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.5,null,"µg/L"]
["110-97-4","Diisopropanolamine ","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",1.6,null,"mg/L"]
["120-12-7","Anthracene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",4,null,"µg/L"]
["120-12-7","Anthracene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.1,null,"µg/L","Phototoxic"]
["123-31-9","4-hydroxyphenol (hydroqinone, quinol)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",4.5,null,"ug/L"]
["126-33-0","Sulfolane","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",50,null,"mg/L"]
["129-00-0","Pyrene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.02,null,"µg/L","Phototoxic"]
["1330-20-7","Xylene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.03,null,"mg/L"]
["1336-36-3","Polychlorinated Biphenyls","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.1,null,"ng/L"]
["14797-55-8(as N)","Nitrate as N","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",32.799999999999997,null,"mg/L"]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.02,null,"mg/L",null,null,"16887-00-6","mg/L",null,null,"<",2]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.04,null,"mg/L",null,null,"16887-00-6","mg/L",">=",2,"<",4]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.06,null,"mg/L",null,null,"16887-00-6","mg/L",">=",4,"<",6]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.08,null,"mg/L",null,null,"16887-00-6","mg/L",">=",6,"<",8]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.1,null,"mg/L",null,null,"16887-00-6","mg/L",">=",8,"<",10]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.2,null,"mg/L",null,null,"16887-00-6","mg/L",">=",10]
["14866-68-3","Chlorate","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",30,null,"mg/L"]
["1634-04-4","Methyl Tertiary-Butyl Ether","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",3.4,null,"mg/L"]
["16887-00-6","Chloride","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",600,null,"mg/L"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.4,null,"mg/L",null,null,"Hardness_as_CaCO3","mg/L",null,null,"<=",10]
["16984-48-8","Fluoride","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",null,null,"mg/L","[-51.73 + 92.57 log10 (hardness*)] × 0.01",null,"Hardness_as_CaCO3","mg/L",">",10]
["206-44-0","Fluoranthene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",4,null,"µg/L"]
["206-44-0","Fluoranthene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.2,null,"µg/L","Phototoxic"]
["260-94-6","Acridene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",3,null,"µg/L"]
["260-94-6","Acridene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.05,null,"µg/L","Phototoxic"]
["32598-13-3","PCB77","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.04,null,"ng/L"]
["32598-14-4","PCB105","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.09,null,"ng/L"]
["32774-16-6","PCB169","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.06,null,"ng/L"]
["42617-16-3","Chlorophyll","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",100,null,"mg/m2"]
["50-32-8","Benzo[a]pyrene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.01,null,"µg/L"]
["56-55-3","Benz[a]anthracene ","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.1,null,"µg/L"]
["57465-28-8","PCB126","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",2.5000000000000001E-4,null,"ng/L"]
["57-63-6","17a-ethinylestradiol (EE2)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.75,null,"ng/L"]
["64743-03-9","Total of all other phenols","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",50,null,"ug/L"]
["71-43-2","Benzene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",40,null,"ug/L"]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.1,null,"mg/L",null,null,"pH_field","-",">=",6.5,null,null,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.02,null,"mg/L",null,null,"pH_field","-",">=",4,"<=",4.5999999999999996,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",2.1000000000000001E-2,null,"mg/L",null,null,"pH_field","-",">=",4.7,"<=",4.8,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",2.1999999999999999E-2,null,"mg/L",null,null,"pH_field","-",">=",4.9000000000000004,"<=",4.9000000000000004,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",2.3E-2,null,"mg/L",null,null,"pH_field","-",">=",5,"<=",5,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",2.4E-2,null,"mg/L",null,null,"pH_field","-",">=",5.0999999999999996,"<=",5.0999999999999996,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",2.5000000000000001E-2,null,"mg/L",null,null,"pH_field","-",">=",5.2,"<=",5.2,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",2.7E-2,null,"mg/L",null,null,"pH_field","-",">=",5.3,"<=",5.3,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",2.9000000000000001E-2,null,"mg/L",null,null,"pH_field","-",">=",5.4,"<=",5.4,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",3.1E-2,null,"mg/L",null,null,"pH_field","-",">=",5.5,"<=",5.5,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",3.3000000000000002E-2,null,"mg/L",null,null,"pH_field","-",">=",5.6,"<=",5.6,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",3.5999999999999997E-2,null,"mg/L",null,null,"pH_field","-",">=",5.7,"<=",5.7,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",3.9E-2,null,"mg/L",null,null,"pH_field","-",">=",5.8,"<=",5.8,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",4.2999999999999997E-2,null,"mg/L",null,null,"pH_field","-",">=",5.9,"<=",5.9,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",4.7E-2,null,"mg/L",null,null,"pH_field","-",">=",6,"<=",6,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",5.1999999999999998E-2,null,"mg/L",null,null,"pH_field","-",">=",6.1,"<=",6.1,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",5.8999999999999997E-2,null,"mg/L",null,null,"pH_field","-",">=",6.2,"<=",6.2,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",6.6000000000000003E-2,null,"mg/L",null,null,"pH_field","-",">=",6.3,"<=",6.3,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",7.3999999999999996E-2,null,"mg/L",null,null,"pH_field","-",">=",6.4,"<=",6.4,false,true]
["7439-89-6","Iron","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",1,null,"mg/L"]
["7439-89-6","Iron","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.35,null,"mg/L"]
["7439-92-1","Lead","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",3,null,"ug/L",null,null,"Hardness_as_CaCO3","mg/L",null,null,"<=",8]
["7439-92-1","Lead","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",null,null,"ug/L","e^[1.273 ln (hardness*) -1.460]",null,"Hardness_as_CaCO3","mg/L",">",8]
["7439-96-5","Manganese","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",null,null,"mg/L","≤ 0.01102 hardness** + 0.54","≤"]
["7439-98-7","Molybdenum","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",2,null,"mg/L"]
["7440-22-4","Silver","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.1,null,"ug/L",null,null,"Hardness_as_CaCO3","mg/L",null,null,"<=",100]
["7440-22-4","Silver","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",3,null,"ug/L",null,null,"Hardness_as_CaCO3","mg/L",">",100]
["7440-38-2","Arsenic (total)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",5,null,"ug/L"]
["7440-42-8","Boron","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",1.2,null,"mg/L"]
["7440-43-9","Cadmium","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",null,null,"ug/L","e^[1.03 * ln(Hss) - 5.274]"]
["7440-48-4","Cobalt","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",110,null,"ug/L"]
["7440-50-8","Copper (total)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",null,null,"ug/L","0.094 hardness** + 2","≤","Hardness_as_CaCO3","mg/L",null,null,null,50]
["7440-50-8","Copper (total)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",null,null,"ug/L","0.094 hardness** + 2","≤","Hardness_as_CaCO3","mg/L",">",50]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",33,null,"ug/L",null,null,"Hardness_as_CaCO3","mg/L",null,null,"<=",90]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",null,null,"ug/L","33 + 0.75(hardness** - 90)",null,"Hardness_as_CaCO3","mg/L",">",90]
["7664-41-7 (as N)","Ammonia as N","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",null,null,"mg/L","Tables 3 and 4"]
["7723-14-0","Phosphorous","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",15,5,"ug/L","Lakes"]
["7782-50-5","Chlorine","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",100,null,"ug/L"]
["83-32-9","Acenaphthene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",6,null,"µg/L"]
["85-01-8","Phenanthrene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",0.3,null,"µg/L"]
["86-73-7","Fluorene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",12,null,"µg/L"]
["91-20-3","Naphthalene","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",1,null,"µg/L"]
["Chlorophenols(All)","Chlorophenols","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",null,null,"ug/L","refer to Table 1"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",43,null,"num/100mL","Shellfish harvesting - 90th percentile","≤"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",14,null,"num/100mL","Shellfish harvesting - median","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",11,null,"num/100mL","Shellfish harvesting - 90th percentile","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",4,null,"num/100mL","Shellfish harvesting - median","≤"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",43,null,"num/100mL","Shellfish harvesting - 90th percentile","≤"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",14,null,"num/100mL","Shellfish harvesting - median","≤"]
["Gas_Pressure","Total Gas Pressure","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",76,null,"mmHg",null,"≤"]
["Temp","Temperature","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",18,null,"oC"]
["TURBIDITY","Turbidity","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",null,null,"NTU","Compare to Background"]
["WAD_CYANIDE","Weak-acid Dissociable Cyanide","Water","BC Approved WQG - Fresh Water Aquatic Life (Max)",10,null,"ug/L"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Industrial (Max)",1.5,null,"mg/L"]
["7439-97-6","Mercury","Water","BC Approved WQG - Industrial (Max)",1,null,"ug/L"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Industrial (Max)",0,null,"num/100mL","(dairy food processing) no treatment"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Industrial (Max)",10,null,"num/100mL","(dairy food processing) disinfection only - 90th percentile","≤"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Industrial (Max)",100,null,"num/100mL","(dairy food processing) partial treatment - 90th percentile","≤"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Industrial (Max)",385,null,"num/100mL","other industries - geometric mean","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Industrial (Max)",0,null,"num/100mL","(dairy food processing) no treatment"]
["Enterococci","Enterococci","Water","BC Approved WQG - Industrial (Max)",3,null,"num/100mL","(dairy food processing) disinfection only - 90th percentile","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Industrial (Max)",25,null,"num/100mL","(dairy food processing) partial treatment - 90th percentile","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Industrial (Max)",100,null,"num/100mL","other industries - geometric mean","≤"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Industrial (Max)",0,null,"num/100mL","(dairy food processing) no treatment"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Industrial (Max)",10,null,"num/100mL","(dairy food processing) disinfection only - 90th percentile","≤"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Industrial (Max)",100,null,"num/100mL","(dairy food processing) partial treatment - 90th percentile","≤"]
["Pseudomonasaeruginos","Pseudomonas aeruginosa","Water","BC Approved WQG - Industrial (Max)",10,null,"num/100mL","other industries - 7th percentile","≤"]
["110-97-4","Diisopropanolamine ","Water","BC Approved WQG - Irrigation Water Supply (Max)",3.9,null,"mg/L"]
["126-33-0","Sulfolane","Water","BC Approved WQG - Irrigation Water Supply (Max)",8.4,null,"mg/L"]
["1336-36-3","Polychlorinated Biphenyls","Water","BC Approved WQG - Irrigation Water Supply (Max)",0.5,null,"ug/L"]
["14797-55-8(as N)","Nitrate as N","Water","BC Approved WQG - Irrigation Water Supply (Max)",100,null,"mg/L"]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Irrigation Water Supply (Max)",10,null,"mg/L"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Irrigation Water Supply (Max)",2,null,"mg/L"]
["7429-90-5","Aluminium (total)","Water","BC Approved WQG - Irrigation Water Supply (Max)",5,null,"mg/L",null,null,"pH_field","-",null,null,null,null,true,false]
["7439-92-1","Lead","Water","BC Approved WQG - Irrigation Water Supply (Max)",200,null,"ug/L","Neutral and alkaline fine-textured soils"]
["7439-92-1","Lead","Water","BC Approved WQG - Irrigation Water Supply (Max)",400,null,"ug/L","All other soils"]
["7439-97-6","Mercury","Water","BC Approved WQG - Irrigation Water Supply (Max)",2,null,"ug/L"]
["7439-98-7","Molybdenum","Water","BC Approved WQG - Irrigation Water Supply (Max)",0.05,null,"mg/L","Well drained soil"]
["7440-38-2","Arsenic (total)","Water","BC Approved WQG - Irrigation Water Supply (Max)",100,null,"ug/L"]
["7440-42-8","Boron","Water","BC Approved WQG - Irrigation Water Supply (Max)",0.5,null,"mg/L","Blackberry","<"]
["7440-42-8","Boron","Water","BC Approved WQG - Irrigation Water Supply (Max)",1,0.5,"mg/L","Peach, cherry, plum, grape, cowpea, onion, garlic, sweet potato, wheat, barley, sunflower, mung bean, sesame, lupin, strawberry, Jerusalem artichoke, kidney bean, lima bean"]
["7440-42-8","Boron","Water","BC Approved WQG - Irrigation Water Supply (Max)",2,1,"mg/L","Red pepper, pea, carrot, radish, potato, cucumber"]
["7440-42-8","Boron","Water","BC Approved WQG - Irrigation Water Supply (Max)",4,2,"mg/L","Lettuce, cabbage, celery, turnip, Kentucky bluegrass, oat, corn, artichoke, tobacco, mustard, clover, squash, muskmelon"]
["7440-42-8","Boron","Water","BC Approved WQG - Irrigation Water Supply (Max)",6,4,"mg/L","Sorghum, tomato, alfalfa, purple vetch, parsley, red beet, sugar beet"]
["7440-42-8","Boron","Water","BC Approved WQG - Irrigation Water Supply (Max)",15,6,"mg/L","Asparagus"]
["7440-50-8","Copper (total)","Water","BC Approved WQG - Irrigation Water Supply (Max)",200,null,"ug/L"]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Irrigation Water Supply (Max)",1000,null,"ug/L","soil pH less than 6"]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Irrigation Water Supply (Max)",2000,null,"ug/L","soil pH equal to or greater than 6 and less than 7"]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Irrigation Water Supply (Max)",5000,null,"ug/L","soil pH greater than or equal to 7"]
["7782-50-5","Chlorine","Water","BC Approved WQG - Irrigation Water Supply (Max)",1000,null,"ug/L"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Irrigation Water Supply (Max)",77,null,"num/100mL","Crops eaten raw - geometric mean","≤"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Irrigation Water Supply (Max)",385,null,"num/100mL","public/livestock access - geometric mean","≤"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Irrigation Water Supply (Max)",1000,null,"num/100mL","general irrigation - geometric mean","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Irrigation Water Supply (Max)",20,null,"num/100mL","Crops eaten raw - geometric mean","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Irrigation Water Supply (Max)",100,null,"num/100mL","public/livestock access - geometric mean","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Irrigation Water Supply (Max)",250,null,"num/100mL","general irrigation - geometric mean","≤"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Irrigation Water Supply (Max)",200,null,"num/100mL","Crops eaten raw - geometric mean","≤"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Irrigation Water Supply (Max)",1000,null,"num/100mL","general irrigation - geometric mean","≤"]
["Pseudomonasaeruginos","Pseudomonas aeruginosa","Water","BC Approved WQG - Irrigation Water Supply (Max)",10,null,"num/100mL","public/livestock access - 75th percentile","≤"]
["TURBIDITY","Turbidity","Water","BC Approved WQG - Irrigation Water Supply (Max)",null,null,"NTU","Compare to Background"]
["110-97-4","Diisopropanolamine ","Water","BC Approved WQG - Livestock Water Supply (Max)",38,null,"mg/L"]
["126-33-0","Sulfolane","Water","BC Approved WQG - Livestock Water Supply (Max)",14,null,"mg/L"]
["14797-55-8(as N)","Nitrate as N","Water","BC Approved WQG - Livestock Water Supply (Max)",100,null,"mg/L"]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Livestock Water Supply (Max)",10,null,"mg/L"]
["14866-68-3","Chlorate","Water","BC Approved WQG - Livestock Water Supply (Max)",3,null,"mg/L"]
["1634-04-4","Methyl Tertiary-Butyl Ether","Water","BC Approved WQG - Livestock Water Supply (Max)",11,null,"mg/L"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Livestock Water Supply (Max)",1.5,null,"mg/L","Dairy Cows, Breeding Stock - long-lived animals"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Livestock Water Supply (Max)",2,null,"mg/L","High F- diets, mineral or bone meal, feed additives"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Livestock Water Supply (Max)",4,null,"mg/L","Normal diet"]
["25167-80-0(sum)","Monochlorophenols","Water","BC Approved WQG - Livestock Water Supply (Max)",185,null,"ug/L","Toxicity for Lactating Animals (High Temperatures & High Water Intake Rates)"]
["25167-80-0(sum)","Monochlorophenols","Water","BC Approved WQG - Livestock Water Supply (Max)",1854,null,"ug/L","Toxicity for Non-Lactating Animals (Normal Temperatures & Low Water Intake Rates)"]
["25167-81-1(sum)","Dichlorophenols","Water","BC Approved WQG - Livestock Water Supply (Max)",46,null,"ug/L","Toxicity for Lactating Animals (High Temperatures & High Water Intake Rates)"]
["25167-81-1(sum)","Dichlorophenols","Water","BC Approved WQG - Livestock Water Supply (Max)",460,null,"ug/L","Toxicity for Non-Lactating Animals (Normal Temperatures & Low Water Intake Rates)"]
["25167-82-2(sum)","Trichlorophenols","Water","BC Approved WQG - Livestock Water Supply (Max)",21,null,"ug/L","Toxicity for Lactating Animals (High Temperatures & High Water Intake Rates)"]
["25167-82-2(sum)","Trichlorophenols","Water","BC Approved WQG - Livestock Water Supply (Max)",210,null,"ug/L","Toxicity for Non-Lactating Animals (Normal Temperatures & Low Water Intake Rates)"]
["25167-83-3(sum)","Tetrachlorophenols","Water","BC Approved WQG - Livestock Water Supply (Max)",41,null,"ug/L","Toxicity for Lactating Animals (High Temperatures & High Water Intake Rates)"]
["25167-83-3(sum)","Tetrachlorophenols","Water","BC Approved WQG - Livestock Water Supply (Max)",410,null,"ug/L","Toxicity for Non-Lactating Animals (Normal Temperatures & Low Water Intake Rates)"]
["25167-83-4(sum)","Pentachlorophenols","Water","BC Approved WQG - Livestock Water Supply (Max)",17.5,null,"ug/L","Toxicity for Lactating Animals (High Temperatures & High Water Intake Rates)"]
["25167-83-4(sum)","Pentachlorophenols","Water","BC Approved WQG - Livestock Water Supply (Max)",175,null,"ug/L","Toxicity for Non-Lactating Animals (Normal Temperatures & Low Water Intake Rates)"]
["7429-90-5","Aluminium (total)","Water","BC Approved WQG - Livestock Water Supply (Max)",5,null,"mg/L",null,null,"pH_field","-",null,null,null,null,true,false]
["7439-92-1","Lead","Water","BC Approved WQG - Livestock Water Supply (Max)",100,null,"ug/L"]
["7439-97-6","Mercury","Water","BC Approved WQG - Livestock Water Supply (Max)",3,null,"ug/L"]
["7439-98-7","Molybdenum","Water","BC Approved WQG - Livestock Water Supply (Max)",0.08,null,"mg/L","Consuming forages not irrigated or if no Mo containing fertilizers are applied to grow feed consumed by livestock"]
["7439-98-7","Molybdenum","Water","BC Approved WQG - Livestock Water Supply (Max)",0.05,null,"mg/L","All other cases"]
["7440-38-2","Arsenic (total)","Water","BC Approved WQG - Livestock Water Supply (Max)",25,null,"ug/L"]
["7440-42-8","Boron","Water","BC Approved WQG - Livestock Water Supply (Max)",5,null,"mg/L"]
["7440-50-8","Copper (total)","Water","BC Approved WQG - Livestock Water Supply (Max)",300,null,"ug/L"]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Livestock Water Supply (Max)",2000,null,"ug/L"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Livestock Water Supply (Max)",200,null,"num/100mL","General livestock use"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Livestock Water Supply (Max)",0,null,"num/100mL","closely confined (no treatment)"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Livestock Water Supply (Max)",10,null,"num/100mL","closely confined (disinfection only) - 09th percentile","≤"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Livestock Water Supply (Max)",100,null,"num/100mL","closely confined (partial treatment) - 90th percentile","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Livestock Water Supply (Max)",50,null,"num/100mL","General livestock use"]
["Enterococci","Enterococci","Water","BC Approved WQG - Livestock Water Supply (Max)",0,null,"num/100mL","closely confined (no treatment) - 90th percentile"]
["Enterococci","Enterococci","Water","BC Approved WQG - Livestock Water Supply (Max)",3,null,"num/100mL","closely confined (disinfection only) - 09th percentile","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Livestock Water Supply (Max)",25,null,"num/100mL","closely confined (partial treatment) - 90th percentile","≤"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Livestock Water Supply (Max)",200,null,"num/100mL","General livestock use"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Livestock Water Supply (Max)",0,null,"num/100mL","closely confined (no treatment)"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Livestock Water Supply (Max)",10,null,"num/100mL","closely confined (disinfection only) - 90th percentile","≤"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Livestock Water Supply (Max)",100,null,"num/100mL","closely confined (partial treatment) - 90th percentile","≤"]
["NO3+NO2 (as N)","Nitrite + Nitrate as N","Water","BC Approved WQG - Livestock Water Supply (Max)",100,null,"mg/L"]
["TURBIDITY","Turbidity","Water","BC Approved WQG - Livestock Water Supply (Max)",null,null,"NTU","Compare to Background"]
["100-41-4","Ethylbenzene","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",0.25,null,"mg/L"]
["1321-94-4","Methylated naphthalene","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",1,null,"µg/L"]
["1336-36-3","Polychlorinated Biphenyls","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",0.1,null,"ng/L"]
["14866-68-3","Chlorate","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",5,null,"mg/L"]
["1634-04-4","Methyl Tertiary-Butyl Ether","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",0.44,null,"mg/L"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",1.5,null,"mg/L"]
["218-01-9","Chrysene","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",0.1,null,"µg/L"]
["32598-13-3","PCB77","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",0.04,null,"ng/L"]
["32598-14-4","PCB105","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",0.09,null,"ng/L"]
["32774-16-6","PCB169","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",0.06,null,"ng/L"]
["50-32-8","Benzo[a]pyrene","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",0.01,null,"µg/L"]
["57465-28-8","PCB126","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",2.5000000000000001E-4,null,"ng/L"]
["71-43-2","Benzene","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",110,null,"ug/L"]
["7439-92-1","Lead","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",140,null,"ug/L"]
["7440-22-4","Silver","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",3,null,"ug/L"]
["7440-38-2","Arsenic (total)","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",12.5,null,"ug/L"]
["7440-42-8","Boron","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",1.2,null,"mg/L"]
["7440-50-8","Copper (total)","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",3,null,"ug/L"]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",10,null,"ug/L"]
["7664-41-7 (as N)","Ammonia as N","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",null,null,"mg/L","Table 5"]
["7782-50-5","Chlorine","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",40,null,"ug/L"]
["83-32-9","Acenaphthene","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",6,null,"µg/L"]
["86-73-7","Fluorene","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",12,null,"µg/L"]
["91-20-3","Naphthalene","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",1,null,"µg/L"]
["Chlorophenols(All)","Chlorophenols","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",null,null,"ug/L","refer to Table 1"]
["TURBIDITY","Turbidity","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",null,null,"NTU","Compare to Background"]
["WAD_CYANIDE","Weak-acid Dissociable Cyanide","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (Max)",1,null,"ug/L"]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Recreation and Aesthetics (30 day)",5000,null,"ug/L"]
["100-41-4","Ethylbenzene","Water","BC Approved WQG - Recreation and Aesthetics (Max)",2.3999999999999998E-3,null,"mg/L"]
["14797-55-8(as N)","Nitrate as N","Water","BC Approved WQG - Recreation and Aesthetics (Max)",10,null,"mg/L"]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Recreation and Aesthetics (Max)",1,null,"mg/L"]
["1634-04-4","Methyl Tertiary-Butyl Ether","Water","BC Approved WQG - Recreation and Aesthetics (Max)",0.02,null,"mg/L"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Recreation and Aesthetics (Max)",1.5,null,"mg/L"]
["42617-16-3","Chlorophyll","Water","BC Approved WQG - Recreation and Aesthetics (Max)",50,null,"mg/m2"]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Recreation and Aesthetics (Max)",0.2,null,"mg/L",null,null,"pH_field","-",null,null,null,null,false,true]
["7439-92-1","Lead","Water","BC Approved WQG - Recreation and Aesthetics (Max)",50,null,"ug/L"]
["7439-97-6","Mercury","Water","BC Approved WQG - Recreation and Aesthetics (Max)",1,null,"ug/L"]
["7440-50-8","Copper (total)","Water","BC Approved WQG - Recreation and Aesthetics (Max)",1000,null,"ug/L"]
["7723-14-0","Phosphorous","Water","BC Approved WQG - Recreation and Aesthetics (Max)",10,null,"ug/L"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Recreation and Aesthetics (Max)",385,null,"num/100mL","Secondary contact/crustacean harvesting - geometric mean","≤"]
["E.Coli","Escherichia coli","Water","BC Approved WQG - Recreation and Aesthetics (Max)",77,null,"num/100mL","primary contact - geometric mean","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Recreation and Aesthetics (Max)",100,null,"num/100mL","Secondary contact/crustacean harvesting - geometric mean","≤"]
["Enterococci","Enterococci","Water","BC Approved WQG - Recreation and Aesthetics (Max)",20,null,"num/100mL","primary contact - geometric mean","≤"]
["Faecal_Coliform","Fecal coliforms","Water","BC Approved WQG - Recreation and Aesthetics (Max)",200,null,"num/100mL","primary contact - geometric mean","≤"]
["Pseudomonasaeruginos","Pseudomonas aeruginosa","Water","BC Approved WQG - Recreation and Aesthetics (Max)",10,null,"num/100mL","Secondary contact/crustacean harvesting - 75th percentile","≤"]
["Pseudomonasaeruginos","Pseudomonas aeruginosa","Water","BC Approved WQG - Recreation and Aesthetics (Max)",2,null,"num/100mL","primary contact - 7th percentile","≤"]
["Temp","Temperature","Water","BC Approved WQG - Recreation and Aesthetics (Max)",30,null,"oC"]
["TURBIDITY","Turbidity","Water","BC Approved WQG - Recreation and Aesthetics (Max)",null,null,"NTU","Compare to Background"]
["14797-55-8(as N)","Nitrate as N","Water","BC Approved WQG - Wildlife Water Supply (Max)",100,null,"mg/L"]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Wildlife Water Supply (Max)",10,null,"mg/L"]
["14866-68-3","Chlorate","Water","BC Approved WQG - Wildlife Water Supply (Max)",3,null,"mg/L"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Wildlife Water Supply (Max)",1.5,null,"mg/L"]
["25167-80-0(sum)","Monochlorophenols","Water","BC Approved WQG - Wildlife Water Supply (Max)",185,null,"ug/L","Toxicity for Lactating Animals (High Temperatures & High Water Intake Rates)"]
["25167-80-0(sum)","Monochlorophenols","Water","BC Approved WQG - Wildlife Water Supply (Max)",1854,null,"ug/L","Toxicity for Non-Lactating Animals (Normal Temperatures & Low Water Intake Rates)"]
["25167-81-1(sum)","Dichlorophenols","Water","BC Approved WQG - Wildlife Water Supply (Max)",46,null,"ug/L","Toxicity for Lactating Animals (High Temperatures & High Water Intake Rates)"]
["25167-81-1(sum)","Dichlorophenols","Water","BC Approved WQG - Wildlife Water Supply (Max)",460,null,"ug/L","Toxicity for Non-Lactating Animals (Normal Temperatures & Low Water Intake Rates)"]
["25167-82-2(sum)","Trichlorophenols","Water","BC Approved WQG - Wildlife Water Supply (Max)",21,null,"ug/L","Toxicity for Lactating Animals (High Temperatures & High Water Intake Rates)"]
["25167-82-2(sum)","Trichlorophenols","Water","BC Approved WQG - Wildlife Water Supply (Max)",210,null,"ug/L","Toxicity for Non-Lactating Animals (Normal Temperatures & Low Water Intake Rates)"]
["25167-83-3(sum)","Tetrachlorophenols","Water","BC Approved WQG - Wildlife Water Supply (Max)",41,null,"ug/L","Toxicity for Lactating Animals (High Temperatures & High Water Intake Rates)"]
["25167-83-3(sum)","Tetrachlorophenols","Water","BC Approved WQG - Wildlife Water Supply (Max)",410,null,"ug/L","Toxicity for Non-Lactating Animals (Normal Temperatures & Low Water Intake Rates)"]
["25167-83-4(sum)","Pentachlorophenols","Water","BC Approved WQG - Wildlife Water Supply (Max)",17.5,null,"ug/L","Toxicity for Lactating Animals (High Temperatures & High Water Intake Rates)"]
["25167-83-4(sum)","Pentachlorophenols","Water","BC Approved WQG - Wildlife Water Supply (Max)",175,null,"ug/L","Toxicity for Non-Lactating Animals (Normal Temperatures & Low Water Intake Rates)"]
["7429-90-5","Aluminium (total)","Water","BC Approved WQG - Wildlife Water Supply (Max)",5,null,"mg/L",null,null,"pH_field","-",null,null,null,null,true,false]
["7439-92-1","Lead","Water","BC Approved WQG - Wildlife Water Supply (Max)",100,null,"ug/L"]
["7439-98-7","Molybdenum","Water","BC Approved WQG - Wildlife Water Supply (Max)",0.05,null,"mg/L"]
["7440-38-2","Arsenic (total)","Water","BC Approved WQG - Wildlife Water Supply (Max)",25,null,"ug/L"]
["7440-42-8","Boron","Water","BC Approved WQG - Wildlife Water Supply (Max)",5,null,"mg/L"]
["7440-50-8","Copper (total)","Water","BC Approved WQG - Wildlife Water Supply (Max)",300,null,"ug/L"]
["NO3+NO2 (as N)","Nitrite + Nitrate as N","Water","BC Approved WQG - Wildlife Water Supply (Max)",100,null,"mg/L"]
["TURBIDITY","Turbidity","Water","BC Approved WQG - Wildlife Water Supply (Max)",null,null,"NTU","Compare to Background"]

{"sheet":"30 Day","index":4,"n_rows":112,"n_cols":17,"rows_kept":112,"cut":false,"hidden":false,"merged":[]}
["Project:","|All","0|0","Table:","[zRef_Environmental_Standards]",null,"Style:","EnviroStandards","HasLocs"]
["ODBC:","FileDSN=C:\\Users\\nicktumney.EARTHSCIENCE\\Documents\\_ESdat\\esdatonline-ca.dsn;UID=?UID;Password=3CvpNGg4;Trusted_Connection=no",null,"Parent Tables:","zRef_Matrix_Types,zRef_Chemistry_Lookup",null,"OnlineBaseURL:","http://online-ca.esdat.net"]
["|All"]
["ChemCode","ChemName","MatrixType","ActionLevelSource","ActionLevel","ActionLevel_Min","Units","Comments","ActionLevel_Prefix","Conditional_ChemCode1","Conditional_ChemCode1_Units","Conditional_ChemCode1_Min_Value_Prefix","Conditional_ChemCode1_Value_Min","Conditional_ChemCode1_Max_Value_Prefix","Conditional_ChemCode1_Value_Max","Applies_To_Total_Result","Applies_To_Filtered_Result"]
["16887-00-6","Chloride","Water","BC Approved WQG - Drinking Water Supply (30 day)",250,null,"mg/L"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Drinking Water Supply (30 day)",1,null,"mg/L"]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Drinking Water Supply (30 day)",5000,null,"ug/L"]
["57-63-6","17a-ethinylestradiol (EE2)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.5,null,"ng/L"]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.05,null,"mg/L",null,null,"pH_Field","-",">=",6.5,null,null,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",5.0000000000000001E-3,null,"mg/L",null,null,"pH_Field","-",">=",4,"<=",4.5,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",6.0000000000000001E-3,null,"mg/L",null,null,"pH_Field","-",">=",4.5999999999999996,"<=",4.9000000000000004,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",7.0000000000000001E-3,null,"mg/L",null,null,"pH_Field","-",">=",5,"<=",5.0999999999999996,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",8.0000000000000002E-3,null,"mg/L",null,null,"pH_Field","-",">=",5.2,"<=",5.2,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",8.9999999999999993E-3,null,"mg/L",null,null,"pH_Field","-",">=",5.3,"<=",5.3,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.01,null,"mg/L",null,null,"pH_Field","-",">=",5.4,"<=",5.4,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",1.0999999999999999E-2,null,"mg/L",null,null,"pH_Field","-",">=",5.5,"<=",5.5,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",1.2E-2,null,"mg/L",null,null,"pH_Field","-",">=",5.6,"<=",5.6,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",1.2999999999999999E-2,null,"mg/L",null,null,"pH_Field","-",">=",5.7,"<=",5.7,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",1.4999999999999999E-2,null,"mg/L",null,null,"pH_Field","-",">=",5.8,"<=",5.8,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",1.7999999999999999E-2,null,"mg/L",null,null,"pH_Field","-",">=",5.9,"<=",5.9,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.02,null,"mg/L",null,null,"pH_Field","-",">=",6,"<=",6,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",2.4E-2,null,"mg/L",null,null,"pH_Field","-",">=",6.1,"<=",6.1,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",2.8000000000000001E-2,null,"mg/L",null,null,"pH_Field","-",">=",6.2,"<=",6.2,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",3.3000000000000002E-2,null,"mg/L",null,null,"pH_Field","-",">=",6.3,"<=",6.3,false,true]
["7429-90-5","Aluminium (dissolved)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.04,null,"mg/L",null,null,"pH_Field","-",">=",6.4,"<=",6.4,false,true]
["7664-41-7 (as N)","Ammonia as N","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",null,null,"mg/L","Table 4"]
["16887-00-6","Chloride","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",150,null,"mg/L"]
["7782-50-5","Chlorine","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",2,null,"ug/L"]
["7440-48-4","Cobalt","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",4,null,"ug/L"]
["Colour","Colour","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",5,null,"mg/L Pt","True Color"]
["7440-50-8","Copper","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",2,null,"ug/L",null,"≤","Hardness_as_CaCO3","mg/L",null,null,"<=",50]
["7440-50-8","Copper","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.04,null,"ug/L",null,"≤","Hardness_as_CaCO3","mg/L",">",50]
["DO","Dissolved Oxygen","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",8,null,"mg/L","All life stages other than buried embryo or alevin"]
["DO","Dissolved Oxygen","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",9,null,"mg/L","Water column - Buried embryo / alevin life stages"]
["DO","Dissolved Oxygen","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",6,null,"mg/L","Interstitial water - Buried embryo / alevin life stages"]
["DO_Field","DO (Field)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",8,null,"mg/L","All life stages other than buried embryo or alevin"]
["DO_Field","DO (Field)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",9,null,"mg/L","Water column - Buried embryo / alevin life stages"]
["DO_Field","DO (Field)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",6,null,"mg/L","Interstitial water - Buried embryo / alevin life stages"]
["7439-92-1","Lead (total)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",null,null,"ug/L","3.31 + e(1.273 ln (mean hardness) - 4.704)","≤","Hardness_as_CaCO3","mg/L",">",8]
["7439-96-5","Manganese","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",null,null,"mg/L","0.0044 hardness + 0.605"]
["7439-97-6","Mercury","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.02,null,"ug/L","When MeHg = 0.5% of THg"]
["7439-97-6","Mercury","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.01,null,"ug/L","When MeHg = 1.0% of THg"]
["7439-97-6","Mercury","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",1.25E-3,null,"ug/L","When MeHg = 8.0% of THg"]
["7439-98-7","Molybdenum","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",1,null,"mg/L",null,"≤"]
["14797-55-8(as N)","Nitrate as N","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",3,null,"mg/L"]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.02,null,"mg/L",null,null,"16887-00-6","mg/L",null,null,"<",2]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.04,null,"mg/L",null,null,"16887-00-6","mg/L",">=",2,"<",4]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.06,null,"mg/L",null,null,"16887-00-6","mg/L",">=",4,"<",6]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.08,null,"mg/L",null,null,"16887-00-6","mg/L",">=",6,"<",8]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.1,null,"mg/L",null,null,"16887-00-6","mg/L",">=",8,"<",10]
["14797-65-0(as N)","Nitrite as N","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.2,null,"mg/L",null,null,"16887-00-6","mg/L",">=",10]
["TOC","Organic Carbon","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",null,null,"mg/L","30-day median ± 20% of the  median background concentration "]
["DOC","Organic Carbon","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",null,null,"mg/L","30-day median ± 20% of the  median background concentration "]
["7782-49-2","Selenium","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",2,null,"ug/L"]
["7440-22-4","Silver","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",0.05,null,"ug/L",null,null,"Hardness_as_CaCO3","mg/L",null,null,"<=",100]
["7440-22-4","Silver","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",1.5,null,"ug/L",null,null,"Hardness_as_CaCO3","mg/L",">",100]
["14808-79-8","Sulphate","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",128,null,"mg/L",null,null,"Hardness_as_CaCO3","mg/L",null,null,"<=",30]
["14808-79-8","Sulphate","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",218,null,"mg/L",null,null,"Hardness_as_CaCO3","mg/L",">",30,"<=",75]
["14808-79-8","Sulphate","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",309,null,"mg/L",null,null,"Hardness_as_CaCO3","mg/L",">",75,"<=",180]
["14808-79-8","Sulphate","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",429,null,"mg/L",null,null,"Hardness_as_CaCO3","mg/L",">",180,"<",250]
["14808-79-8","Sulphate","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",null,null,"mg/L","Site specific",null,"Hardness_as_CaCO3","mg/L",">=",250]
["WAD_CYANIDE","Weak-acid Dissociable Cyanide","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",5,null,"ug/L",null,"≤"]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",7.5,null,"ug/L",null,null,"Hardness_as_CaCO3","mg/L",null,null,"<=",90]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Fresh Water Aquatic Life (30 day)",null,null,"ug/L","7.5 + 0.75 x (hardness minus 90)",null,"Hardness_as_CaCO3","mg/L",">",90]
["16984-48-8","Fluoride","Water","BC Approved WQG - Industrial (30 day)",1,null,"mg/L"]
["16887-00-6","Chloride","Water","BC Approved WQG - Irrigation Water Supply (30 day)",100,null,"mg/L"]
["7782-50-5","Chlorine","Water","BC Approved WQG - Irrigation Water Supply (30 day)",3,null,"ug/L"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Irrigation Water Supply (30 day)",1,null,"mg/L"]
["7439-98-7","Molybdenum","Water","BC Approved WQG - Irrigation Water Supply (30 day)",0.01,null,"mg/L","Poorly Drained Soil Cu:Mo ratio is less than 2:1 in the irrigation water (forage crops)","≤"]
["7439-98-7","Molybdenum","Water","BC Approved WQG - Irrigation Water Supply (30 day)",0.02,null,"mg/L","Poorly Drained Soil Cu:Mo ratio is greater than 2:1 in the irrigation water (forage crops)","≤"]
["7439-98-7","Molybdenum","Water","BC Approved WQG - Irrigation Water Supply (30 day)",0.02,null,"mg/L","Well-drained soil (forage crops)","≤"]
["7439-98-7","Molybdenum","Water","BC Approved WQG - Irrigation Water Supply (30 day)",0.03,null,"mg/L","All soils (non-forage crops)","≤"]
["7782-49-2","Selenium","Water","BC Approved WQG - Irrigation Water Supply (30 day)",10,null,"ug/L"]
["16887-00-6","Chloride","Water","BC Approved WQG - Livestock Water Supply (30 day)",600,null,"mg/L"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Livestock Water Supply (30 day)",1,null,"mg/L","Dairy cows, breeding stock - long-lived animals"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Livestock Water Supply (30 day)",1,null,"mg/L","high fluoride diets, mineral or bone meal feed additives"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Livestock Water Supply (30 day)",2,null,"mg/L","normal diet"]
["7782-49-2","Selenium","Water","BC Approved WQG - Livestock Water Supply (30 day)",30,null,"ug/L"]
["7664-41-7 (as N)","Ammonia as N","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",null,null,"mg/L","Table 6"]
["16887-00-6","Chloride","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",null,null,"mg/L","10% of background"]
["7782-50-5","Chlorine","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",3,null,"ug/L"]
["Colour","Colour","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",5,null,"mg/L Pt","True Color"]
["7440-50-8","Copper","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",2,null,"ug/L",null,"≤"]
["DO","Dissolved Oxygen","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",8,null,"mg/L","All life stages other than buried embryo or alevin"]
["DO","Dissolved Oxygen","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",9,null,"mg/L","Water column - Buried embryo / alevin life stages"]
["DO","Dissolved Oxygen","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",6,null,"mg/L","Interstitial water - Buried embryo / alevin life stages"]
["DO_Field","DO (Field)","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",8,null,"mg/L","All life stages other than buried embryo or alevin"]
["DO_Field","DO (Field)","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",9,null,"mg/L","Water column - Buried embryo / alevin life stages"]
["DO_Field","DO (Field)","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",6,null,"mg/L","Interstitial water - Buried embryo / alevin life stages"]
["7439-92-1","Lead (total)","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",2,null,"ug/L"]
["7439-97-6","Mercury","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",0.02,null,"ug/L","When MeHg = 0.5% of THg"]
["7439-97-6","Mercury","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",0.01,null,"ug/L","When MeHg = 1.0% of THg"]
["7439-97-6","Mercury","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",1.25E-3,null,"ug/L","When MeHg = 8.0% of THg"]
["14797-55-8(as N)","Nitrate as N","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",3.7,null,"mg/L"]
["7782-49-2","Selenium","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",2,null,"ug/L"]
["7440-22-4","Silver","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",1.5,null,"ug/L"]
["14808-79-8","Sulphate","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",128,null,"mg/L",null,null,"Hardness_as_CaCO3","mg/L",null,null,"<=",30]
["14808-79-8","Sulphate","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",218,null,"mg/L",null,null,"Hardness_as_CaCO3","mg/L",">",30,"<=",75]
["14808-79-8","Sulphate","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",309,null,"mg/L",null,null,"Hardness_as_CaCO3","mg/L",">",75,"<=",180]
["14808-79-8","Sulphate","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",429,null,"mg/L",null,null,"Hardness_as_CaCO3","mg/L",">",180,"<",250]
["14808-79-8","Sulphate","Water","BC Approved WQG - Marine and Estuarine Aquatic Life (30 day)",null,null,"mg/L","Site specific",null,"Hardness_as_CaCO3","mg/L",">=",250]
["Colour","Colour","Water","BC Approved WQG - Recreation and Aesthetics (30 day)",15,null,"mg/L Pt","True Color"]
["7440-66-6","Zinc (total)","Water","BC Approved WQG - Recreation and Aesthetics (30 day)",5000,null,"ug/L"]
["16887-00-6","Chloride","Water","BC Approved WQG - Wildlife Water Supply (30 day)",600,null,"mg/L"]
["Colour","Colour","Water","BC Approved WQG - Wildlife Water Supply (30 day)",5,null,"mg/L Pt","True Color"]
["16984-48-8","Fluoride","Water","BC Approved WQG - Wildlife Water Supply (30 day)",1,null,"mg/L"]
["7439-97-6","Mercury","Water","BC Approved WQG - Wildlife Water Supply (30 day)",0.02,null,"ug/L","When MeHg = 0.5% of THg"]
["7439-97-6","Mercury","Water","BC Approved WQG - Wildlife Water Supply (30 day)",0.01,null,"ug/L","When MeHg = 1.0% of THg"]
["7439-97-6","Mercury","Water","BC Approved WQG - Wildlife Water Supply (30 day)",1.25E-3,null,"ug/L","When MeHg = 8.0% of THg"]
["TOC","Organic Carbon","Water","BC Approved WQG - Wildlife Water Supply (30 day)",null,null,"mg/L","30-day median ± 20% of the  median background concentration "]
["DOC","Organic Carbon","Water","BC Approved WQG - Wildlife Water Supply (30 day)",null,null,"mg/L","30-day median ± 20% of the  median background concentration "]
["7782-49-2","Selenium","Water","BC Approved WQG - Wildlife Water Supply (30 day)",2,null,"ug/L"]

{"sheet":"MonRoundInfo","index":5,"n_rows":3,"n_cols":1,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["Monitoring_Round"]
["Project_ID"]
["PID"]